**Copper thickness inner layer after processing**

